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	Criteria Met?
	Comments / Drawing Reference

	Public Realm

	Building design provides a variety of textures and details to create visual interest and activate streets and pedestrian-oriented spaces
	
	

	Development incorporates public-realm enhancements (e.g., covered entrances, street furniture, patios, landscaping, lighting, garbage receptacles)
	
	

	Commercial services with limited street transparency (e.g., banks, offices) are located above grade or at the extremities of the Gibsons Landing commercial area
	
	

	Buildings and structures are pedestrian-oriented at the ground level
	
	

	Ground-level pedestrian orientation is achieved through emphasis on fenestration
	
	

	Architectural emphasis, awnings, or step-backs are provided at the first or second storey to impart pedestrian scale
	
	

	Weather protection is provided along pedestrian routes using awnings, arcades, or canopies integral to the building form (maximum 3.5 m above finished grade)
	
	

	Street-level shopfronts are highly transparent and constructed of glass or similar materials
	
	

	Publicly accessible pathways and/or elevators are provided between waterfront walkways and street edges where applicable
	
	

	Pathways have a minimum width of 2.0 m and are designed for universal accessibility where feasible
	
	

	Building design integrates First Nations, marine, heritage, and/or waterfront design elements
	
	

	These design elements are also incorporated into street furniture, landscaping, and/or public art where possible
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	Comments / Drawing Reference

	Building Form and Design

	Building facades facing principal commercial streets or lanes emphasize the first storey to provide pedestrian-scale design
	
	

	Buildings greater than two storeys include a minimum 3.0 m step-back above the second storey
	
	

	Commercial uses facing a street provide all-season weather protection (canopies, awnings, overhangs, vestibules, recessed entrances, etc.)
	
	

	Unobstructed view corridors (minimum 3.0 m wide) are provided at least every 30.0 m to maintain ocean views
	
	

	Building longitudinal axis does not exceed 30.0 m in length when measured at or above 1.0 m above natural grade along Gower Point Road
	
	

	Building massing steps with the natural grade of the land
	
	

	Varied roof heights are provided to create interest in the roofscape and skyline
	
	

	Street and waterfront elevations are articulated into smaller building sections
	
	

	New development or renovations reflect the form and character of the surrounding neighbourhood
	
	

	Historical elements of the building or property are respected and preserved where possible
	
	

	Transitions – Fencing and Landscaping

	Transitions between the waterfront walkway and adjoining properties emphasize landscape elements
	
	

	Marine shoreline landscaping is reviewed by a Qualified Environmental Professional and complies with the ESA DPA
	
	

	Fencing does not exceed 1.2 m in height and is supplemented with plant material
	
	

	Landscaping consists primarily of local indigenous plant species
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	Large areas of non-vegetative materials (e.g., gravel, bark, mulch) are not used
	
	

	Outdoor storage areas, mechanical equipment, waste containers, and parking areas are screened from view
	
	

	Planted trellises are incorporated into non-vegetative screening where possible
	
	

	Buildings and landscaping follow natural site contours and incorporate terraced forms where appropriate
	
	

	Retaining walls are integrated as design features (e.g., walkways, steps, planted habitat, gardens, viewing areas)
	
	

	Architectural Features

	New commercial and mixed-use buildings emphasize individual storefronts and fine-grained facade rhythms
	
	

	Facade widths and rhythms are consistent with surrounding buildings
	
	

	Bright and playful colours are incorporated where appropriate to enhance vibrancy
	
	

	Projected window bays are incorporated where feasible
	
	

	Side-wall windows visible from the street are provided where permitted by code
	
	

	Artistic banners and flags (without logos or advertising) are used to activate the streetscape
	
	

	Signage

	Signage is scaled, oriented, and sited for pedestrian visibility
	
	

	Signage is architecturally coordinated with building design, features, and finishes
	
	

	Signage is integrated into architectural elements (canopies, awnings, pediments, windows, or landscaped frontages)
	
	

	Timber or wood-look materials and metal are used for signage
	
	

	Individual carved and/or hand-painted signs are used where possible
	
	

	Signage is externally illuminated only (no internal illumination)
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	Parking

	Off-street parking is located underground wherever feasible
	
	

	Where surface parking is necessary, it is internal to the development and screened from public view
	
	

	Screening includes walls, fencing, hedging, planting, or a combination of these materials
	
	

	Parking areas and access roads include adequate pedestrian-scale lighting
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