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	Criteria Met? 
	Comments / Drawing Reference

	Building Form & Design

	Building design is compatible with surrounding development and land uses and incorporates visual interest to avoid a monotonous appearance or blank walls
	
	

	Monolithic structures and long expanses of straight walls facing roadways are avoided
	
	

	Walls facing roadways incorporate elements such as windows, entrances, or sloped roofs to add variety and vertical definition
	
	

	Larger buildings are designed to create the impression of smaller blocks or units
	
	

	Buildings and structures are pedestrian-oriented at the ground level
	
	

	Ground-level pedestrian orientation is achieved through fenestration, architectural emphasis, step-backs, or weather protection
	
	

	Weather protection is provided along pedestrian routes using awnings, arcades, or canopies integral to the building form (maximum 3.5 m above finished grade)
	
	

	Buildings are finished in painted or coated metal, wood, or textured concrete rather than untreated flat concrete block
	
	

	Buildings and structures appear permanent in nature and not temporary (e.g., trailers)
	
	

	Exterior lighting is designed to minimize light spill, glare, and sky glow through the use of non-glare, full cut-off fixtures
	
	

	Screening and Landscaping

	Screening and landscaping are provided along property edges adjacent to roadways
	
	

	Screening and landscaping are provided between parking areas, roadways, and buildings
	
	

	Landscaping is used to break up larger parking areas

	
	

	Screening and landscaping are provided between buildings and parking areas
	
	

	Landscaping includes a mix of coniferous and deciduous vegetation, with low plantings and taller tree species at regular intervals
	
	



	
	Criteria Met? 
	Comments / Drawing Reference

	Large areas of bark mulch, bare earth, landscape fabric, gravel, or similar materials are avoided
	
	

	Outdoor and rooftop service installations (mechanical, electrical, etc.) are enclosed with screening structures integrated with building design
	
	

	Mechanical equipment is not visible from street level (except renewable energy equipment such as solar panels or windmills)
	
	

	Where mechanical equipment visibility is unavoidable, planting is used to screen equipment and improve building façade appearance
	
	

	Transitions

	Transitions to adjacent mixed-use or residential properties protect privacy and mitigate noise, glare, and shadow impacts
	
	

	A minimum 3.0 m landscaped buffer is provided where adjacent to residential or mixed-use properties
	
	

	Fencing combined with dense shrub plantings or hedges is provided where appropriate
	
	

	Trees capable of screening up to a 3-storey multi-unit dwelling are provided
	
	

	Commercial buildings are sited to afford maximum privacy to adjacent residential and rural properties
	
	

	Parking

	Parking lots with more than 10 stalls include one landscape island for every 10 stalls
	
	

	Bicycle parking is provided and is conveniently and visibly located adjacent to the main entrance
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